Lab2

Group ID: 20

Nathan Coleman <ndc0002@auburn.edu>

Lucas Saltz <las0029@auburn.edu>

a) Does code work: **Yes.** Tux machines tested on:tux179, tux195

b) Compilation/running instructions:

This project includes a Makefile. To compile, run -$make from this directory (this directory being the one that holds the src directory, the Makefile, etc.

After running make, the compiled .o files reside in the obj/ directory while the linked executables reside in the bin/ directory.

To make only UDPClient, -$make UDPClient

To clean make-related files, -$make clean

Because python is an interpreted language, the .py source code files will need to be run from the src/ directory in which they reside.

**Examples:**

**make**

**python src/UDPServer.py <10030>**

**bin/UDPClient <tux195> <10030> <5> <tux179>**

c) Responses:

d) Bugs: